|  |  |  |  |
| --- | --- | --- | --- |
|  |  | verified |  |
| 1-1 | System shall produce IR signal | simulation |  |
| 1-2 | Signal shall be unique to each button |  | Controllablity |
| 1-3 | Signal shall not harm user for 24 hour continuous useage |  | safety |
| 1-4 | Signal shall not break from dropping 15 feet under | Experiment | Durability |
| 1-5 | Button shall be labeled for each usage | observation |  |
|  | Battery shall be replaceable |  |  |
|  |  |  |  |

Ece362 doc inclass